Date: 08-07-2007

Use Infinity ND:YAG laser: 345 mJ and 50 Hz at 1064-nm (a little lower than before)
(lamp voltage is displayed to be close to the maximum)

Observers:   10:00 ~ 2:00  Cao/Erika 
              2:00 ~ 6:00  Wu/Shuki
            
Weather status: Cloudy, hazy
 
Lidar status:
Power measured at 11:30 am by cao
         355nm  :  1.37 w
         532nm  :  2.18 w 
         1064nm :  2.10 w 
align laser beam (355-532-1064) at 1:00pm by cao
align laser beam (355-532-1064) at 3:40pm by Wu


Power measured at 15:00 am by wu/cao/Leona
         355nm  :  1.2 w
         532nm  :  3.8 w 
         1064nm :  1.57 w 

    
end at 18:00 pm 